Figure 1: Tenth Figure in Lecture 9. Plot of the Deviation of the actual value from the Driver value. The solid line is the LS line fit to these Driver error values. Clearly, the drivers with big loads tend to undercount while the drivers with small loads tend to overcount.